**Commands**

**CheckLiveChanges**

Check Changes from live and make those changes on local server

No Parameters required

Call Import Settings function

**InitializeDevice**

Send Socket connection to devices

Parameters:

Device=device\_id

Status=settings\_status(initialize device,location\_settings,etc)

$command = 'whitelist\_tiings';

$data = '22|' . $key;

**OpenTicketReader**

Send Socket connection to device to open gate

Parameters:

Device=device\_id

$command = 'open\_gate';

$data = '26|' . $key;

**OdSendMessage**

Send Message to OD Device

Parameters:

Device=Device\_id

Message= message

message\_key